**Hardware and Software Requirements for Locked In App**

**Hardware**

Raspberry Pi 3 Model B+

HC-SR04 or HC-SR05 Ultrasonic Distance Sensor

**Software**

Updated Node-RED Server

Flows.json file in repository contains the required flow

Mobile Application